Building Material for 44’/100’

14’ side wall 2/6 construction

Steel on the sidewalls with 42” wainscot Color TBD 7/16” side wall sheathing

Roof will have rafter 2’ on center and 15/32” roof decking with steel.

2’ overhang all the way around the roof edge with soffit.

Interior will be R19 ff insulation and blow in the ceiling R55 with white liner panel steel 5 rows of side wall purlins.

Overhead door will be 6-10’/10 ‘ 1-12’/12’

2 Walk through doors.